# Score layer weighing rules

Tuuli 40%

Elevation 25%

Slope 25%

Soil type 10%

Input layers (min-max)

tuuliatlas\_3MW\_100m\_grid2500m\_transformed\_band1\_clipped

“tuuliatlas\_reclassified@1"\*0.5\*0.4+"elevation\_reclassified@1"\*0.25+"slope\_reclassified@1"\*0.25+"mp200k\_maalajit\_raster\_reclassified@1"\*0.5\*0.1

wind energy production \* 0.4 + elevation \* 0.25 + slope \* 0.25 + soil type \*0.1